# SSERC logo

**SSERC Risk Assessment** (revised version March 2018)

(based on HSE’s INDG 163 ‘Risk assessment - A brief guide to controlling risks in the workplace’)

2 Pitreavie Court, South Pitreavie Business Park, Dunfermline KY11 8UU

tel : 01383 626070 e-mail : enquiries@sserc.org.uk web : [www.sserc.org.uk](http://www.sserc.org.uk)

#

|  |  |
| --- | --- |
| Activity assessed | Neutralising Strong and Weak Acids |
| *Date of assessment* | 30th June 2020 |
| *Date of review (****Step 5****)* |  |
| *School* |  |
| *Department* |  |

| Step 1 | Step 2 | Step 3 | Step 4 |
| --- | --- | --- | --- |
| *List Significant hazards here:* | *Who might be harmed and how?* | *What are you already doing?**What further action is needed?* | *Actions* |
| *by whom?* | *Due date* | *Done* |
| Hydrochloric acid is corrosive and produces corrosive vapour | Technician preparing 2M solution by splashes and/or inhalation. | Wear goggles (EN 166 3 or a face shield and work in a fume cupboard or a well-ventilated lab. |  |  |  |
| 0.1M Hydrochloric acid is of no significant hazard. |  |  |  |  |  |
| Sodium hydroxide is corrosive | Technician preparing 2M solution by splashing. | Wear goggles (EN166 3) and gloves. Be careful of heat evolved during the dissolving. |  |  |  |
| 0.1M sodium hydroxide is of no significant hazard. |  |  |  |  |  |
| Ethanoic acid is corrosive and produces corrosive vapour | Technician preparing 1M solution by splashes and/or inhalation. | Wear goggles (EN 166 3) or a face shield and work in a fume cupboard or a well-ventilated lab. |  |  |  |
| 0.1M Ethanoic acid is of no significant hazard |  |  |  |  |  |
| Universal indicator is flammable. | Technicians while preparing and Teacher/ pupil while using by ignition. | Keep solution away from sources of ignition. |  |  |  |

|  |
| --- |
| **Description of activity:**Plastic Pasteur pipettes are used to carry out a form of simple titration with strong/weak acids against a strong base, pH being monitored by universal indicator. |
| **Additional comments:**The resulting solutions are of low hazard and can be safely washed to waste. |